1. Standard Ganter Install below instructions for G7 go here: [Gantner G7 Install Guide.docx](https://fernwoodfitness-my.sharepoint.com/:w:/g/personal/caroline_smith_fernwoodfitness_com_au/Efk6EArVe9lAh_dNGcY06jkBaqIXvhjllnU2vad6_q5PgA?e=bwqTbE)
2. Open Gat Config Manager
3. Create Project – Club Name
4. Device model should be displayed.
5. Download IP Scanner <https://www.advanced-ip-scanner.com/news/index.php?ID=7713>
6. Run & Scan.
7. Open Command Prompt -type ipconfig/all & take note of Subnet mask & Default Gateway.
8. Choose 240 to 245 from the available IP addresses.
9. Go back to Gat Config Manager
10. Click Configure > Ethernet.
11. Uncheck DHCP.
12. Change IP address & Static Default Gateway to the same IP.
13. Change Static Primary & Secondary to the one listed in Command Prompt.
14. Check Relay 1
15. Default State: No (normally open)
16. General: Enable Emergency Mode
17. Pulse time: Change to 1000 > click ok
18. Scan Device > Check details match
19. Change name to: 24/7 Front Door > Click save
20. Go to Exerp > Client > Create Client > Centre: TBD by club > Name 24/7 Controller > Client Type: Controller
21. Install Exerp Controller <https://fernwood.exerp.com/installer/download/controller/windows/x86_64/exerp-installer.exe>
22. Run Installer and paste in Controller code.
23. Once Controller install is completed check Services to see that Controller is listed as running on the device.
24. Go to Exerp > Client > Change to Controller.
25. Add device > Driver is Gantner GAT access > Next.
26. Put same IP address as set on Gat Config Manager
27. Switch relay: 3-4
28. Enable Emergency log to: True > Finish.
29. Go to Configuration in Exerp > Access > Resources > Create.
30. Name: 24/7 Front Door
31. Type: Change from Room to Gate
32. Attend: tick Attenable
33. Access Group: Gym Access 24/7
34. Override for Staff > tick
35. Click ok & make sure it says Created > Click activate.
36. Go to Gates > Create.
37. Name: 24/7 Front Door
38. Client: Computer Name [Controller] select
39. Device: gantnergataccess6xxx(tcp) select > Ok
40. Access points: Create > Name: 24/7 Front Door > Save > Edit
41. Actions > Add > Name 24/7 Front Door
42. Resources > Attend > 24/7 Front Door
43. Gate > tick Open gate > 24/7 Front Door
44. Options > tick Handbag check & Block incomplete agreement > click ok
45. Specific sources > add > Select Device directly it will load Gantner device.
46. Then action 24/7 Front Door > click ok & save. This will default to inactive change to active.
47. Log out of Exerp to refresh changes.
48. Log back in, go to Menu > Client > Controller > Devices > click on Gantner Device > Start > Refresh – device should now be listed as started. If it isn’t, log out of Exerp completely and go to Services & check the Controller & start it.
49. You can then set up the OMNIKEY Assign & Attend readers <https://www.hidglobal.com/Download-EULA?headless=&regionfree=&nid=32909>
50. Assign a 24/7 FOB.
51. Test Front door & Attend PC.